Earth filling 225mm thick

# G.L G.L

225

Inlet pipe 100mm dia.

75mm thick RCC precast slab covering

Inlet pipe 100mm dia.

825

Rough Stone Dry

Packing 300mm thick for sides

40mm Broken stone filling 150mm thick for

750

1350

750

sides & 300mm for bottom

150 150

## 150 1350



1650

150

# SECTION

PLAN

Note: All Dimensions are in Millimeters unless otherwise mentioned



Andhra Pradesh State Housing Corporation Ltd

Nirmaan Bhavan, Auto Nagar, Vijayawada-520007

PROPOSED MAGIC SOAKPIT MODEL DRAWING FOR HOUSES IN YSR JAGANANNA HOUSING LAYOUTS